# sscc option

#### Syntax

sscc option { user-ip-mask-override | send-calling-station-id | send-local-qos-profile-config }

no sscc option

#### Release Information

Command introduced in JunosE Release 10.2.0.

send-calling-station-id keyword added in JunosE Release 11.1.0.

send-local-qos-profile-config keyword added in JunosE Release 11.2.0.

#### Description

When used with the user-ip-mask-override option, enables the user IP address mask to be sent to the Policy Decision Point (PDP) in place of the interface IP address mask for a virtual router. If user IP address mask is not available, then the interface IP address mask is sent. The no version disables user IP address mask override.

When used with the send-calling-station-id option, enables the calling station ID to be sent to the PDP for a virtual router. The no version disables the option to send the calling station ID.

When used with the send-local-qos-profile-config option, enables the local QoS profile attachment information to be sent to the PDP for a virtual router. The no version disables the option to send the local QoS profile attachment information.

#### Options

- user-ip-mask-override—Enables user IP address mask to be sent to PDP.
- send-calling-station-id—Enables calling station ID to be sent to PDP.
- send-local-qos-profile-config—Enables local QoS profile attachment information to be sent to the PDP.

#### Mode

Global Configuration