# ip pim rp-address

#### Syntax

[ no ] ip pim rp-address ipAddress [ ipAccessList ] [ override ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies a static PIM group–to–RP mapping. The no version clears the mapping from this interface.

#### Options

- ipAddress—IP address of the router you want to designate as an RP router
- ipAccessList—Name of the IP access list that specifies which multicast groups use this RP
- override—Specifies that this static RP mapping has priority over group-to-RP mappings learned by auto-RP

#### Mode

Global Configuration