# version

#### Syntax

version { 1 | 2 }

no version

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the global RIP version. The no version reverts to the default value, RIP version 1. Use the ip rip receive and ip rip send version commands to specify the RIP version for a specific interface.

#### Options

- 1—RIP version 1
- 2—RIP version 2

#### Mode

Address Family Configuration, Router Configuration