# vlan advisory-tx-speed

#### Syntax

vlan advisory-tx-speed speed

no vlan advisory-rx-speed

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Sets an advisory connect (Tx) speed that the LAC sends in the Tx connect speed to the LNS. The no version restores the default behavior, in which the Tx speed is not sent to the LNS.

#### Options

- speed—Speed in the range 0–2147483647 kbps; 0 indicates no advisory speed setting

#### Mode

Profile Configuration, Subinterface Configuration