# ip ospf network

#### Syntax

ip ospf network { broadcast | non-broadcast | point-to-point }

no ip ospf network

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the OSPF network type to something other than the default for the network medium. The no version restores the default value for the medium.

#### Options

- broadcast—Sets the network type to broadcast
- non-broadcast—Sets the network type to NBMA
- point-to-point—Sets the network type to point-to-point

#### Mode

Interface Configuration, Subinterface Configuration