# Supported Interface Types for QoS Profiles

Each QoS profile command begins with a keyword that designates an interface type.

Table 14 lists the interface types and the commands that you can use with them.

Table 14: Interface Types and Supported Commands

Interface Type | Queue | Node | Group | Shadow Node
--- | --- | --- | --- | ---
atm | ✓ | ✓ | ✓ | ✓
atm-vc | ✓ | ✓ | – | ✓
atm-vp | ✓ | ✓ | – | ✓
bridge | ✓ | ✓ | – | ✓
ethernet | ✓ | ✓ | ✓ | ✓
fr-vc | ✓ | ✓ | – | ✓
ip | ✓ | ✓ | – | ✓
ip-tunnel | ✓ | ✓ | – | ✓
ipv6 | ✓ | ✓ | – | ✓
l2tp-session | ✓ | ✓ | – | ✓
l2tp-tunnel | ✓ | ✓ | – | ✓
lsp | ✓ | ✓ | – | ✓
serial | ✓ | ✓ | ✓ | ✓
server-port | ✓ | ✓ | ✓ | ✓
svlan | ✓ | ✓ | – | ✓
vlan | ✓ | ✓ | – | ✓

#### Related Documentation

- Configuring a QoS Profile
- Configuring Shadow Nodes