# path ds3 mdl carrier

#### Syntax

[ no ] path pathChannel ds3 ds3Channel mdl carrier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies that a DS3 signal is used in the carrier environment. This command applies to a DS3 over channelized SONET interface. The no version restores the default situation, in which an interface does not operate in the carrier environment.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the path

#### Mode

Controller Configuration