# DHCP Local Server Configuration Tasks

This section covers the configuration tasks for equal-access and standalone modes. Perform the appropriate procedure:

1. For both equal-access and standalone modes, configure the DHCP local server.

   See Configuring AAA Authentication for DHCP Local Server Standalone Mode for a sample configuration.

2. For standalone mode, optionally configure the router to use AAA authentication for DHCP requests from subscribers.

   See Configuring AAA Authentication for DHCP Local Server Standalone Mode for a sample configuration.

3. For non-PPP equal access, configure the router to work with the SRC software.

   See Configuring the Router to Work with the SRC Software for a sample configuration.