Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

# Configuring Fragmentation on Multiclass MLPPP Interfaces

You can configure fragmentation on a multiclass MLPPP interface with the same fragment size as that of the MLPPP interface.

Before you configure fragmentation on the multiclass MLPPP interface:

- Ensure that fragmentation is enabled on the MLPPP interface.

  See Configuring MLPPP Fragmentation and Reassembly in Chapter 8, Configuring Multilink PPP.

To configure fragmentation on a multiclass MLPPP interface:

- Specify the QoS traffic classes to be fragmented.

  - To configure fragmentation on multilink classes in a dynamic profile:

    host1(config-profile)#ppp multilink multiclass fragmentation best-effort voice otherData video

  - To configure fragmentation on multilink classes in a static MLPPP interface:

    host1(config-if)#ppp multilink multiclass fragmentation best-effort voice otherData video

  The order of the QoS traffic classes does not affect the execution of the command.

  | Note: You must include the best-effort traffic class in the ppp multilink multiclass fragmentation command, or the command fails.

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

#### Published: 2011-03-28

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out