# Network Management Tools

You can use different management tools to configure the system to meet the specific networking requirements.

## CLI Management

The CLI provides fully developed and automated configuration and status functionality through a local RS-232 port, Telnet, or SSH via any reachable network. For a full discussion of the CLI, see JunosE System Basics Configuration Guide, Chapter 2, Command-Line Interface.

## SNMP MIB Management

The system offers a complete SNMP interface for configuration, status, and alarm reporting. The system supports both Standard and Enterprise MIBs (Management Information Bases). The Juniper Networks E Series Enterprise MIB is ASN.1 notated for easy importing into third-party SNMP management applications. For more information, see JunosE System Basics Configuration Guide, Chapter 4, Configuring SNMP.

## NMC-RX Device Management System

The NMC-RX application provides a global method of managing all routers, line modules, and ports through a graphical user interface.