# ip atm-vc

#### Syntax

ip ipAddress atm-vc vcd broadcast

no ip ipAddress atm-vc vcd

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Associates a protocol and address to a specific virtual circuit. The no version removes the association.

#### Options

- ipAddress—IP address to be associated with the virtual circuit
- vcd—Number in the range 1–2147483647; virtual circuit descriptor; an identifier for the VC in other commands
- broadcast—Specifies that the circuit should participate in broadcast operations

#### Mode

Map List Configuration