# mpls bandwidth

#### Syntax

{ ip rsvp | mpls } bandwidth bandwidth

no { ip rsvp | mpls } bandwidth

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the total bandwidth reservable for MPLS on the interface. The no version restores the default value, 0.

#### Options

- ip rsvp—Specifies keyword for compatibility with non–E Series implementations of MPLS
- mpls—Specifies JunosE MPLS implementation
- bandwidth—Reservable bandwidth in kilobits per second, a value in the range 1–10000000

#### Mode

Interface Configuration