# show adjustment-factor

#### Syntax

show adjustment-factor [ adsl1 | adsl2 | adsl2+ | vdsl | vdsl2 | sds ]

#### Release Information

Command introduced in JunosE Release 9.1.0.

#### Description

Displays the configured QoS adjustment factor that is applied to the ANCP-reported downstream and upstream data rate for all DSL line types or for the specified DSL line types.

#### Options

- dslType—Type of DSL line for which the QoS adjustment rate is displayed: adsl1, adsl2, adsl2+, vdsl, vdsl2, or sds

#### Mode

L2C Configuration