# convergence-factor

#### Syntax

convergence-factor convergenceFactor

no convergence-factor

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies the convergence factor for all simple shared shapers on the router. The convergence factor determines how quickly the dynamic shaping rate converges with the calculated dynamic shaping rate, and is expressed as a percentage of the available bandwidth. The no version removes the specified convergence factor from all simple shared shapers on the router.

#### Options

- convergenceFactor—Percentage value in the range 0–99; default value is 50

#### Mode

QoS Shared Shaper Control Configuration

#### Related Documentation

- Configuring Simple Shared Shaper Algorithm Variables