# graceful-restart helper-abort-topology-change

#### Syntax

graceful-restart helper-abort-topology-change { any | non-externals }

no graceful-restart helper-abort-topology-change

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the OSPFv2 or OSPFv3 helper router to cease help to a restarting router under the specified conditions. However, the router continues to act as helper for subsequent graceful restart requests. The no version turns off the graceful restart helper capability.

#### Options

- any—Abandons the helper role when any LSA changes during the restart
- non-externals—Abandons the helper role only when any nonexternal LSA changes during the restart

#### Mode

Router Configuration