# Monitoring ATM Cross-Connects for Layer 2 Services over MPLS

#### Purpose

Display all ATM cross-connects (passthrough connections between local subinterfaces).

#### Action

To display ATM cross-connects:

    host1#show mpls cross-connects atm
                 Cate Peak
    VC-ID  Encap gory Rate Interface  VPI VCI Status
    ------ ----- ---- ---- ---------- --- --- ------
    600001 AAL5  UBR     0 ATM6/0.101   0 101 Up
                           ATM6/2.101   0 101 Up
    600002 AAL5  UBR     0 ATM6/0.102   0 102 Up
                           ATM6/2.102   0 102 Up
    2 local connection(s) found

#### Meaning

Table 105 lists the show mpls cross-connects atm command output fields

Table 105: show mpls cross-connects atm Output Fields

Field Name | Field Description
--- | ---
VC-ID | VC ID number of the connection
Encap | Administered encapsulation method based on what was configured with the atm pvc command
Category | Configured service category
Peak Rate | Send and receive peak rate, in Kbps
Interface | Specifier and status of the first subinterface that makes up the local cross-connect
VPI | Virtual path identifier of the first subinterface
VCI | Virtual channel identifier of the first subinterface
Status | Current state of the connection

#### Related Documentation

- show mpls cross-connects atm