# priority burst

#### Syntax

priority priorityValue burst burstSize

no priority priorityValue burst

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Sets the burst size for each priority. The no version returns to the default value.

#### Options

- priorityValue–Hi-Green-IC, Hi-Green-SC, Hi-Yellow-IC, Hi-Yellow-SC, Lo-Green-IC, Lo-Green-SC, Lo-Yellow-IC, Lo-Yellow-SC
- burstSize—Number of packets, in the range 32–65535; 0 denotes no burst size: default value is equal to half of the configured maximum rate

#### Mode

DoS Protection Group Configuration