# Monitoring Routes Downloaded by the RADIUS Route-Download Server

#### Purpose

Display information about the routes that are downloaded by the RADIUS route-download server.

Use the optional detail keyword to display more detailed information about the downloaded routes.

#### Action

To display information about the routes that are downloaded by the RADIUS route-download server:

    host1#show aaa route-download routes
    96000 downloaded routes

To display detailed information about the routes that are downloaded by the RADIUS route-download server:

    host1#show aaa route-download routes detail
    Prefix/Length      Type        NextHop      Dst/Met  Intf   Tag
    ---------------  --------  ---------------  -------  -----  ---
    192.168.1.1/32   Access-P  255.255.255.255  254/2    null0  0
    192.168.1.5/32   Access-P  255.255.255.255  254/2    null0  0
    192.168.1.9/32   Access-P  255.255.255.255  254/2    null0  0
    192.168.1.13/32  Access-P  255.255.255.255  254/2    null0  0
    192.168.1.17/32  Access-P  255.255.255.255  254/2    null0  0
    192.168.1.21/32  Access-P  255.255.255.255  254/2    null0  0

#### Meaning

Table 18 lists the show aaa route-download routes command output fields.

Table 18: show aaa route-download routes Output Fields

Field Name | Field Description
--- | ---
downloaded routes | Number of current downloaded routes
Prefix/Length | IP address prefix and mask information for downloaded routes
Type | Type of downloaded routes; Access-P indicates routes downloaded from the RADIUS route-download server
NextHop | IP address of the next hop
Dst/Met | Administrative distance and number of hops for the route
Tag | Tag assigned to downloaded routes
Intf | Interface type and specifier

#### Related Documentation

- show aaa route-download routes