# Creating Policy Lists for IP

The following example creates an IP policy list named routeForABCCorp. For information about creating the CLACLs and rate-limit profile used in this example, see the previous sections.

1. Create the policy list routeForABCCorp.
   host1(config)#ip policy-list routeForABCCorp host1(config-policy-list)#
2. Create the classification group for the CLACL named ipCLACL10 and assign the precedence to the classification group.
   host1(config-policy-list)#classifier-group ipCLACL10 precedence 75 host1(config-policy-list-classifier-group)#
3. Add a rule that specifies a group of forwarding solutions based on classifier list ipCLACL10.
   host1(config-policy-list-classifier-group)#forward next-hop 192.0.2.12 order 10 host1(config-policy-list-classifier-group)#forward next-hop 192.0.100.109
   order 20 host1(config-policy-list-classifier-group)#forward next-hop 192.120.17.5 order 30 host1(config-policy-list-classifier-group)#forward interface ip 3/1 order 40
4. Add a rule that sets a ToS byte value of 125 for packets based on classifier list ipCLACL10.
   host1(config-policy-list-classifier-group)#mark tos 125
5. Add a rule that uses rate-limit profile ipRLP25.
   host1(config-policy-list-classifier-group)#rate-limit-profile ipRLP25
6. Exit Classifier Group Configuration mode for ipCLACL10, then create a new classification group for classifier list ipCLACL20. Add a rule that filters packets based on classifier list ipCLACL20.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group ipCLACL20 precedence 125 host1(config-policy-list-classifier-group)#filter
7. Exit Policy List Configuration mode to save the configuration.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#exit host1(config)#
8. Display the policy list.

       host1#show policy-list routeForABCCorp

                                         Policy Table
                                         ------ -----
       IP Policy routeForABCCorp
          Administrative state: enable
          Reference count:      0
          Classifier control list: ipCLACL10, precedence 75
             forward
                Virtual-router: default
                List:
                  next-hop 192.0.2.12, order 10, rule 2 (active)
                  next-hop 192.0.100.109, order 20, rule 3 (reachable)
                  next-hop 192.120.17.5, order 30, rule 4 (reachable)
                  interface ip3/1, order 40, rule 5
             mark tos 125
             rate-limit-profile ipRLP25
          Classifier control list: ipCLACL20, precedence 125
             filter

#### Related Documentation

- ip policy-list