# system

#### Description

System management and monitoring

#### Emergency

None

#### Alert

None

#### Critical

Line module ping failure threshold exceeded; test failure on line module or standby SRP module; test failure on line module or standby SRP module

#### Error

Error on line module or standby SRP module; critical subsystem failure condition (NVS, power, fan, network timing, temperature); unrecognized module type; module ID mismatch; line module memory reduction; line module bandwidth misconfiguration; unrecoverable file system synchronization errors; software incompatibility issue

#### Warning Log

Noncritical subsystem failure condition (heap/CPU utilization, NVS, network timing); unexpected software error; recoverable file system synchronization errors; file system out of synchronization notification; NVS subsystem redundancy size mismatch; line module ID block misconfigured

#### Notice Log

Subsystem failure condition abatement (heap/CPU utilization, NVS, power, fan, network timing, temperature); new module announcement; module revision mismatch; module upgraded or downgraded (ECC/non-ECC); module online or offline

#### Info

Synchronization start, complete; line module set timing failed (not necessarily an error); NVS volume flush

#### Debug

Module state change; module memory announcement; redundancy role changes; server role changes; module enable, disable, or clear notification; file system synchronization (normal operation); line module timing source set failure (not necessarily an error); image protection notification

#### Filter

slot slotNumber

- slot—Logs events for a specific slot
- slotNumber—Number of slot for which you want to log events