# lacp port-priority

#### Syntax

lacp port-priority portPriority

no lacp port-priority

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the priority for an Ethernet member link, also known as an Ethernet port, in an IEEE 802.3ad link aggregation group (LAG) bundle. The member link with the lowest numerical priority value has the highest priority. The Ethernet member link with the highest priority is selected first to join the LAG bundle. The no version restores the default priority value, 32768.

#### Options

- portPriority—Priority value; integer in the range 0–65535; default value is 32768

#### Mode

Interface Configuration