# switch-profile

#### Syntax

switch-profile profileName

no switch-profile

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

From Domain Map Tunnel Configuration mode, applies the specified L2TP tunnel switch profile to sessions associated with an AAA domain map. From Tunnel Group Tunnel Configuration mode, applies the specified L2TP tunnel switch profile to sessions associated with an AAA tunnel group. An L2TP tunnel switch profile defines the L2TP tunnel switching behavior for the interfaces to which this profile is assigned. The no version removes the tunnel switch profile assignment from the AAA domain map or AAA tunnel group.

#### Options

- profileName—Name of the tunnel switch profile; a string of up to 64 alphanumeric characters

#### Mode

Domain Map Tunnel Configuration, Tunnel Group Tunnel Configuration