Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# show vlan subinterface

#### Syntax

show vlan subinterface [ interfaceType interfaceSpecifier ] [ mac-address ] [ filter ]

To display summary information:

show vlan subinterface summary

To display by VLAN ID or S-VLAN ID:

show vlan subinterface { svlan s-vlanIdValue | vlan } { vlanIdValue | any }
[ mac-address ] [ filter ]

To display VLAN subinterfaces that are created based on agent-circuit-identifier information:

show vlan subinterface [ interfaceType interfaceSpecifier | svlan s-vlanIdValue ] agent-circuit-identifier [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
s-vlan keyword and s-vlanIdValue variable added in JunosE Release 7.1.0.
vlan keyword and vlanIdValue variable added in JunosE Release 7.1.0.
any and mac-address keywords added in JunosE Release 7.1.0.
agent-circuit-identifier keyword added in JunosE Release 7.3.0.

#### Description

Displays configuration and status information for a specified VLAN subinterface or for all VLAN subinterfaces configured on the router. Alternatively, you can use the summary keyword to display only brief summary information for all VLAN interfaces. You can also display information about the VLAN IDs or S-VLAN IDs for the specified VLAN subinterface.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers:
  - atm
  - fastEthernet
  - gigabitEthernet
  - lag
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- mac-address—Displays VLAN subinterfaces configured with unique MAC addresses
- filter—See Filtering show Commands
- summary—Displays only the total number of VLAN subinterfaces and the total number of VLAN major interfaces configured on the router
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- vlanIdValue—VLAN ID number in the range 0–4095
- any—Specifies the VLAN ID as a wildcard
- agent-circuit-identifier—Specifies VLAN subinterfaces that are created based on agent-circuit-identifier information

#### Mode

Privileged Exec, User Exec

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out