# aps events

#### Syntax

aps events list [ list ]*

no aps events

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Enables line modules to deliver APS events to the necessary SNMP traps. You can configure notification for specific events. The no version disables the delivery of APS events from line modules to SNMP traps.

#### Options

- list—One of the following APS events:
  - all—Configures notification of all APS events
  - channel-mismatch—Configures notification of APS channel mismatches
  - feplf—Configures notification of APS far-end protection line failures
  - mode-mismatch—Configures notification of APS mode mismatches
  - psbf—Configures notification of APS protection signal byte failures
  - switchover—Configures notification of APS switchovers
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration