# mroute port limit

#### Syntax

mroute port portNumber limit limitValue

no mroute port portNumber limit

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures a limit on the number of outgoing interfaces (OIFs) containing IPv4 or IPv6 mroutes, across different virtual routers, on a port. The no version removes any OIF port limits.

#### Options

- portNumber—Port number in the form slot/port.
- limitValue—Limit on the number of outgoing interfaces containing IPv4 or IPv6 mroutes, across different virtual routers, on a port. The default is no limit.

#### Mode

Global Configuration