# Monitoring Status of Dial-out Sessions

#### Purpose

Display the status of dial-out sessions.

This command displays aspects of the dial-out state machine and details about the dial-out routes themselves. This section presents sample output. The actual output on your router may differ significantly.

#### Action

To display all sessions within the current virtual router context:

    host1#show l2tp dial-out session
    Session           Status
    ---------         ---------
    10.10.1.1         connected
    10.10.2.1          dormant

To display detailed information about a particular session, specify the trigger IP address for the session:

    host1#show l2tp dial-out session 10.1.1.1
    Session 10.1.1.1
    Operational status: dormant

To display aggregate counts for dial-out sessions in each of the possible operational and administrative states:

    host1#show l2tp dial-out session summary

To display detailed configuration, state, and statistics:

    host1#show l2tp dial-out session detail

To display information about the operational or administrative state:

    host1#show l2tp dial-out session state connecting

To display dial-out information across all virtual routers

    host1#show l2tp dial-out session allVirtualRouters

| Note: The level of a user’s permission determines the use of the allVirtualRouters option. For example, if you have permission to view only the current virtual router, then that is all that is displayed when you enter a command.

#### Meaning

Table 97 lists the show l2tp dial-out session command output fields.

Table 97: show l2tp dial-out session Output Fields

Field Name | Field Description
--- | ---
Session | IP address of the session
Status | Current status of the session
Operational status | Current operational status of session

#### Related Documentation

- For detailed information about operational states, see Dial-Out Operational States
- show l2tp dial-out session