# mpls rsvp signalling hello graceful-restart restart-time

#### Syntax

{ ip | mpls } rsvp signalling hello graceful-restart restart-time restartTime

no { ip | mpls } rsvp signalling hello graceful-restart restart-time

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Configures the restart time for RSVP-TE graceful restart for all interfaces that have RSVP-TE enabled. The no version restores the default value.

#### Options

- ip—Specifies alternative keyword for compatibility with non–E Series implementations
- restartTime—Total time in milliseconds for the sender to gracefully restart RSVP-TE and to re-establish hello communication with RSVP-TE neighbors; in the range 60000–3600000; default value is 60000

#### Mode

Global Configuration