# mpls traffic-eng administrative-weight

#### Syntax

mpls traffic-eng administrative-weight weight

no mpls traffic-eng administrative-weight

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the administrative weight for the interface. The no version restores the default value, which matches the IGP-determined weight (cost).

#### Options

- weight—Administrative weight, a value in the range 0–4294967295 supersedes any weight conferred upon the link by the IGP

#### Mode

Interface Configuration, Subinterface Configuration