# node

#### Syntax

[ no ] { typeOfInterface | set | superset } node [ group trafficClassGroup | scheduler-profile
schedulerProfileName ]*

#### Release Information

Command introduced before JunosE Release 7.1.0.
svlan keyword added in JunosE Release 7.1.0.

set and superset keywords added in JunosE Release 9.2.0.

#### Description

Specifies that a scheduler node be configured for each interface of the given interface type. The no version removes this rule from the QoS profile.

#### Options

- typeOfInterface—Interface types for scheduler nodes to be configured: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, server-port, svlan, vlan
- set—Configures the node for an interface set
- superset—Configures the node for an interface superset
- trafficClassGroup—Name of the traffic class group
- schedulerProfileName—Name of the scheduler profile
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

QoS Profile Configuration

#### Related Documentation

- Configuring a QoS Profile
- Configuring Shadow Nodes
- Configuring a Basic Parameter Definition for QoS Administrators
- Attaching a QoS Profile to an Interface Superset or an Interface Set