# adjustment-factor

#### Syntax

adjustment-factor dslType value

no adjustment-factor dslType

#### Release Information

Command introduced in JunosE Release 9.1.0.

#### Description

Configures an adjustment factor that is applied globally to the ANCP-reported downstream and upstream data rate for all subscribers of a particular DSL line type. The adjusted data rate results in an accurate QoS shaping rate. The no version restores the default, wherein the rate is not adjusted.

#### Options

- dslType—Type of DSL subscriber line for which the data rate is adjusted by the specified QoS adjustment factor: adsl1, adsl2, adsl2+, vdsl, vdsl2, or sds
- value—QoS adjustment factor applied to upstream or down stream data rates for the DSL type; a percentage in the range 1–100

#### Mode

L2C Configuration