# path ds3 framing

#### Syntax

path pathChannel ds3 ds3Channel framing framingType

no path pathChannel ds3 ds3Channel framing

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the framing format for a DS3 signal. This command applies to a DS3 over channelized SONET interface. The no version restores the default value.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the path
- framingType—Choose one of the following:
  - c-bit—Default; specifies C-bit parity framing
  - m23—Specifies M23 multiplexer framing

#### Mode

Controller Configuration