# atm oam flush

#### Syntax

[ no ] atm oam flush [ alarm-cells ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the router to ignore all OAM cells received on an ATM interface, and to stop sending OAM cells on this interface. OAM performs fault management and performance management functions on an ATM interface. The no version disables OAM flush on the interface.

#### Options

- alarm-cells—Causes the router to ignore only AIS and RDI cells and to accept all other OAM cells

#### Mode

Interface Configuration