# retransmit

#### Syntax

retransmit retries

no retransmit

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the maximum number of times a router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default value.

#### Options

- retries—Number of retries, in the range 0–100; default value is 3

#### Mode

RADIUS Configuration