# Monitoring VRF Routing Protocols

#### Purpose

Display information about the routing protocols associated with the VRF

#### Action

To display information about OSPF routing protocol associated with the VRF

    host1:pe1#show ip protocols vrf pe13
    Routing Protocol is “ ospf 1" with Router ID 13.13.13.1
      Distance is 110
    Redistributing: bgp
      Address Summarization:
        None
      Routing for Networks:
        13.13.13.0/255.255.255.0 area 0.0.0.0

#### Meaning

Table 96 lists the show ip protocols command output fields.

Table 96: show ip protocols Output Fields

Field Name | Field Description
--- | ---
Routing Protocol | Protocol configured for routing
BGP
Redistributing | Protocol to which BGP is redistributing routes
Default local preference | Local preference value
IGP synchronization | Status of IGP synchronization: enabled, disabled
Always compare MED | Status of multiexit discrimination: enabled, disabled
Router flap damping | Status of route dampening: enabled, disabled
Administrative Distance | External, internal, and local administrative distances
Neighbor Address | IP address of the BGP neighbor
Neighbor Incoming/Outgoing update distribute list | Number of the access list for outgoing routes
Neighbor Incoming/Outgoing update prefix list | Number of the prefix list for incoming or outgoing routes
Neighbor Incoming/Outgoing update prefix tree | Number of the prefix tree for incoming or outgoing routes
Neighbor Incoming/Outgoing update filter list | Number of filter list for incoming routes
Routing for Networks | The network for which BGP is currently injecting routes
IS-IS
System Id | 6-byte value of the router
IS-Type | Routing type of the router: Level 1, Level 2
Distance | Administrative distance for IS-IS learned routes
Address Summarization | Aggregate addresses defined in the routing table for multiple groups of addresses at a given level or routes learned from other routing protocols
Routing for Networks | Network for which IS-IS is currently injecting routes
OSPF
Router ID | OSPF process ID for the router
Distance | Administrative distance for OSPF learned routes
Redistributing | Protocol to which OSPF is redistributing routes
Address Summarization | Aggregate addresses defined in the routing table for multiple groups of addresses at a given level or routes learned form other routing protocols
Routing for Networks | Network for which OSPF is currently injecting routes
RIP
Router Administrative State | RIP protocol state. Enable means it is allowed to send and receive updates. Disable means that it may be configured but it is not allowed to run yet.
System Version | RIP versions allowed for sending and receiving RIP updates. The system version is currently set to RIP1, which sends RIP version 1 but will receive version 1 or 2. If the version is set to RIP2, the system will send and receive version 2 only. The default is configured for RIP1.
Update interval | Current setting of the update timer (in seconds)
Invalid after | Current setting of the invalid timer (in seconds)
hold down time | Current setting of the hold down timer (in seconds)
flushed interval | Current setting of the flush timer (in seconds)
Filter applied to outgoing route update | Access list applied to outgoing RIP route updates
Filter applied to incoming route update | Access list applied to incoming RIP route updates
Global route map | Route map that specifies all RIP interfaces on the router
Distance | Value added to RIP routes added to the IP routing table. The default is 120.
Interface | Interface type on which RIP protocol is running
Redistributing | Protocol to which RIP is redistributing routes
Routing for Networks | Network for which RIP is currently injecting routes

#### Related Documentation

- show ip protocols