# rtr schedule restart-time

#### Syntax

rtr schedule rtrIndex restart-time restartValue

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the interval at which the RTR probe restarts, in seconds. There is no no version.

#### Options

- rtrIndex—Number of the operation to be configured, in the range 1–4294967295; no default
- restartValue—Interval in seconds until test restarts, in the range 0–2147483647; default value is 0, which specifies no restart after the test finishes

#### Mode

Global Configuration