# ip nat translation max-entries

#### Syntax

ip nat translation max-entries maximumEntryNumber

no ip nat translation max-entries

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the maximum number of translation entries per virtual router (that is, address bindings, not translation rules) that the translation table can contain in global configuration mode. The no version removes the configured limit.

#### Options

- maximumEntryNumber—Maximum number of translation entries in the current virtual router; default value is no limit

#### Mode

Global Configuration