# Resetting PIM Counters and Mappings

You can use the clear ipv6 pim commands to reset PIM counters and mappings.

clear ipv6 pim interface

- Use to clear the counters for multicast packet statistics on all interfaces or a specified interface.
- Specify an interface type and identifier, such as atm 3/0 to clear the counters on that interface. For details about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.
- If you do not specify an interface, the router clears the counters on all interfaces.
- Example
  host1#clear ipv6 pim interface atm 3/0.5 count
- There is no no version.
- See clear ipv6 pim interface.

clear ipv6 pim remote-neighbor

- Use to clear the counters for remote neighbor statistics on all interfaces or the specified interface.
- Specify the IP address of an interface to clear the counters for that interface.
- If you do not specify an interface, the router clears the counters on all interfaces.
- Example
  host1#clear ipv6 pim remote-neighbor 1001::1 count
- There is no no version.
- See clear ipv6 pim remote-neighbor.