# ha

#### Description

High availability messages

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Accessing redundancy mode not supported on the standby SRP; changing redundancy mode not supported on the standby SRP; high availability disabled due to state error; error encountered during the transition from one high availability state to another when stateful line module switchover is performed

#### Warning Log

High availability for SRP and line modules disabled due to incompatible release on standby; high availability for SRP and line modules disabled due to user initiated disable

#### Notice Log

High availability for SRP and line modules disabled due to standby down; high availability is now active

#### Info

None

#### Debug

None

#### Filter

None