# baseline ppp interface

#### Syntax

baseline ppp interface { atm | fastEthernet | gigabitEthernet | serial | mlppp | pos } interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

fastEthernet and gigabitEthernet keywords added in JunosE Release 11.0.0

#### Description

Sets a statistics baseline for PPP interfaces. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- atm—Specifies an ATM interface
- fastEthernet—Specifies a Fast Ethernet interface
- gigabitEthernet—Specifies a Gigabit Ethernet interface
- mlppp—Specifies an MLPPP interface
- pos—Specifies a POS interface
- serial—Specifies a serial interface
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec