# Triggering ANCP Line Configuration

Use the l2c line-configuration command to trigger line configuration to the access node. Issuing this command sends a GSMP port management message to the access node. This message enables the B-RAS to configure a service profile name on an access loop.

| Note: Before issuing the l2c line-configuration command, a profile must already be configured locally on the access node.

l2c line-configuration

- Use to trigger a GSMP port management message to the access node. This message enables the B-RAS to configure a service profile name on an access loop.
- Example
  host1#l2c line-configuration interface atm 2/0.11 profile1
- There is no no version.
- See l2c line-configuration.