# Monitoring QoS Configurations for 802.3ad Link Aggregation Groups

To monitor Ethernet configurations for QoS:

- Monitoring the QoS Configuration of Fast Ethernet, Gigabit Ethernet, and 10-Gigabit Ethernet Interfaces
- Monitoring the QoS Configuration of IEEE 802.3ad Link Aggregation Group Bundles
- Monitoring the QoS Configuration of IP Interfaces
- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the Configuration of QoS Port-Type Profiles
- Monitoring the Configuration of QoS Profiles
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers