# show ipv6 pim sparse-mode sg-state

#### Syntax

show ipv6 pim sparse-mode sg-state
[ group groupAddress [ source sourceAddress ] | rp rpAddress ] [ count ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information for each SG entry that PIM sparse mode knows about.

#### Options

- groupAddress—IPv6 address of a multicast group
- sourceAddress—IPv6 address of a multicast source
- rpAddress—IPv6 address of an RP router
- count—Displays the number of SG entries
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec