# Index

A B C D E F G H I J L M N P Q R S T U V

A

> access lists, IP
>   specifying multicast groups
> access lists, IPv6
>   specifying multicast groups
> advertising DVMRP routes 1, 2
> assert messages
> assigning multicast groups 1, 2
> auto-RP router
>   PIM sparse mode
>   PIM sparse-dense mode

B

> baseline commands
>   baseline ip dvmrp
>   baseline ip igmp
>   baseline ip igmp-proxy interface
>   baseline ipv6 mld
>   baseline ipv6 mld-proxy interface
> BFD (Bidirectional Forwarding Detection)
>   RIP, configuring for 1, 2
> BGP multicasting 1, 2

C

> Class D IPv4 addresses
> clear ip commands
>   clear ip dvmrp route
>   clear ip mroute 1, 2
>   clear ip pim auto-rp
>   clear ip pim interface count 1, 2
>   clear ip pim remote-neighbor count
> clear ipv6 commands
>   clear ipv6 mroute
>   clear ipv6 pim remote-neighbor count
> conventions
>   notice icons
>   text and syntax
> customer support
>   contacting JTAC

D

> data MDT, creating
> data path failure
>   detecting RIP 1, 2
> debug commands
>   debug ip pim
>   debug ipv6 pim
> default MDT, creating
> detecting RIP data path failure 1, 2
> disable command
> disable-dynamic-redistribute command
>   DVMRP
> disabling dynamic route redistribution
>   DVMRP
> Distance Vector Multicast Routing Protocol. See DVMRP
> documentation set
>   comments on
> downstream interface 1, 2
> DRs (designated routers)
>   PIM routing 1, 2
> DVMRP (Distance Vector Multicast Routing Protocol)
>   advertising routes 1, 2
>   configuring
>     limits
>     summary addresses
>   default router, configuring
>   deleting routes
>   enabling
>     on a virtual router
>     on an interface
>   exchanging unicast routes
>   filtering reports
>   metric
>   monitoring
>   neighbors
>   overview
>   pruning
>   summary addresses
>   tunnels
>   using with IGMP
>   using with PIM 1, 2
> dynamic route redistribution, disabling
>   in DVMRP

E

> encapsulation commands
>   encapsulation vlan 1, 2
> exchanging DVMRP unicast routes

F

> filtering
>   DVMRP reports

G

> group membership
>   queries 1, 2
>   reports 1, 2

H

> hardware multicast packet replication
>   monitoring 1, 2
>   OIF mapping 1, 2
>   overview 1, 2
> hello interval
>   PIM 1, 2, 3, 4, 5, 6, 7, 8, 9
> hold time
>   PIM sparse mode
> hop count

I

> IGMP (Internet Group Management Protocol)
>   configuring
>   disabling 1, 2
>   enabling 1, 2
>   limiting groups on interfaces
>   monitoring 1, 2
>   performing host functions
>   querier
>   removing
>   specifying version 1, 2, 3
> igmp commands
>   igmp disable
>   igmp promiscuous
> IGMP proxy
>   configuring
>   enabling
>   monitoring
>   version
> IGMP reports, accepting
> IGP (interior gateway protocol)
> importing routes. See redistributing routes
> Internet Group Management Protocol. See IGMP
> investigating IP multicast routes
> IP addresses
>   class D
>   for multicasting
> ip commands
>   ip block-multicast-sources
>   ip multicast-routing 1, 2, 3
>   ip multicast-routing disable-rpf-check 1, 2
>   ip multicast-routing permanent-mroute
>   ip route-type
>   ip rpf-route
>   ip unnumbered 1, 2
>   mroute port limit 1, 2, 3, 4
> ip dvmrp commands See also show ip dvmrp commands
>   ip dvmrp 1, 2
>   ip dvmrp accept-filter
>   ip dvmrp announce-list
>   ip dvmrp auto-summary
>   ip dvmrp disable
>   ip dvmrp metric-offset
>   ip dvmrp route-limit
>   ip dvmrp routehog-notification
>   ip dvmrp summary-address
>   ip dvmrp unicast-routing
> ip igmp commands See also show ip igmp commands
>   ip igmp
>   ip igmp access-group
>   ip igmp access-source-group 1, 2, 3
>   ip igmp group limit
>   ip igmp immediate-leave
>   ip igmp last-member query-interval
>   ip igmp promiscuous
>   ip igmp querier
>   ip igmp querier-timeout
>   ip igmp query-interval
>   ip igmp query-max-response-time
>   ip igmp robustness
>   ip igmp ssm-map enable
>   ip igmp ssm-map static
>   ip igmp static-exclude
>   ip igmp static-group
>   ip igmp static-include
>   ip igmp version 1, 2, 3
>   ip igmp-proxy
>   ip igmp-proxy unsolicited-report-interval
>   ip igmp-proxy V1-router-present-time
> ip multicast commands
>   ip multicast admission-bandwidth-limit
>   ip multicast ioa-packet-replication
>   ip multicast-routing bandwidth-map
> IP multicast groups
>   assigning to an interface
>   identifying
>   leaving
>   maintaining membership of
>   reporting
>   specifying
> IP multicast interfaces, monitoring
> IP multicast routes
> IP multicasting
>   benefits of
>   deleting routes
>   enabling
>   M-BONE
>   monitoring
> ip pim commands See also show ip pim commands
>   ip pim
>   ip pim bsr-candidate
>   ip pim data-mdt
>   ip pim group-address-pool
>   ip pim join-filter
>   ip pim query-interval
>   ip pim rp-address
>   ip pim rp-candidate
>   ip pim send-rp-announce
>   ip pim send-rp-discovery scope
>   ip pim sparse-mode graceful-restart-duration
>   ip pim spt-threshold
> ip rip commands
>   ip rip bfd-liveness-detection 1, 2
> IP tunnels
>   monitoring
> ipv6 commands See also show ipv6 commands
>   ip route-type
>   ipv6 block-multicast-sources
>   ipv6 mld robustness
>   ipv6 multicast-routing
>   ipv6 multicast-routing disable-rpf-check
>   ipv6 multicast-routing permanent-route
>   ipv6 rpf-route
> ipv6 mld commands See also show ipv6 mld commands
>   ipv6 mld
>   ipv6 mld access-group
>   ipv6 mld access-source-group
>   ipv6 mld apply-oif-map
>   ipv6 mld explicit-tracking
>   ipv6 mld group limit
>   ipv6 mld immediate-leave
>   ipv6 mld last-member query-interval
>   ipv6 mld oif-map
>   ipv6 mld querier-timeout
>   ipv6 mld query-interval
>   ipv6 mld query-max-response-time
>   ipv6 mld ssm-map enable
>   ipv6 mld ssm-map static
>   ipv6 mld static-exclude
>   ipv6 mld static-group
>   ipv6 mld static-include
>   ipv6 mld version 1, 2, 3
>   ipv6 mld-proxy
>   ipv6 mld-proxy unsolicited-report-interval
>   ipv6 mld-proxy version
> IPv6 multicast
>   benefits of
>   deleting routes
>   enabling
>   monitoring
> ipv6 multicast commands
>   ipv6 multicast admission-bandwidth-limit
>   ipv6 multicast ioa-packet-replication
>   ipv6 multicast-routing bandwidth-map
> IPv6 multicast groups
>   assigning to an interface
>   identifying
>   leaving
>   maintaining membership of
>   reporting
>   specifying
> ipv6 pim commands See also show ipv6 pim commands
>   ipv6 pim
>   ipv6 pim bsr-candidate
>   ipv6 pim join-filter
>   ipv6 pim query-interval
>   ipv6 pim rp-address
>   ipv6 pim rp-candidate
>   ipv6 pim spt-threshold

J

> join messages 1, 2

L

> leave group membership messages 1, 2
> leaving an IP multicast group
> leaving an IPv6 multicast group
> limiting IGMP groups on interfaces
> limiting MLD groups on interfaces
> liveness detection
>   RIP and BFD 1, 2

M

> M-BONE (multicast backbone of the Internet)
> manuals
>   comments on
> MDT (Multicast Distribution Tree)
>   creating with default MDT
> mdt commands
>   mdt-data-delay
>   mdt-data-holddown
>   mdt-data-timeout
>   mdt-interval
> metric
>   DVMRP
> MLD (Multicast Listener Discovery)
>   configuring
>   disabling 1, 2
>   enabling 1, 2
>   limiting groups on interfaces
>   monitoring
>   performing host functions
>   removing
>   specifying version 1, 2
> mld disable command
> MLD proxy
>   configuring
>   enabling
>   monitoring
>   version
> mrinfo requests, support for
> mtrace command
> multicast
>   IP. See IP multicasting
>   IPv6. See IPv6 multicast
> Multicast Distribution Tree. See MDT
> multicast group port limit command 1, 2
> Multicast Listener Discovery. See MLD
> multicast VPNs
>   creating with data MDTs
>   creating with the default MDT
>   overview

N

> neighbors, DVMRP
> notice icons

P

> PIM (Protocol Independent Multicast) See also PIM dense mode, PIM sparse mode, PIM sparse-dense mode
>   displaying events 1, 2
>   enabling
>     on a virtual router 1, 2
>     on an interface 1, 2
>   monitoring 1, 2, 3, 4
>   removing 1, 2
>   resetting counters and mappings 1, 2
>   using with DVMRP 1, 2
>   using with IGMP
>   using with MLD
> PIM dense mode 1, 2, See also PIM
> pim disable command 1, 2
> PIM SM. See PIM sparse mode
> PIM sparse mode
>   configuring auto-RP router
>   joining groups
>   pruning
>   remote neighbors, configuring 1, 2, 3, 4
>   setting a threshold 1, 2
>   timers 1, 2
> PIM sparse-dense mode
>   configuring auto-RP router
>   overview
> PIM SSM (PIM source-specific multicast)
>   enabling 1, 2
>   requirements for IGMPv3
>   requirements for MLDv2
> Protocol Independent Multicast. See PIM
> prune messages 1, 2

Q

> query-interval command

R

> reachability commands
>   IP multicast
> redistribute command
>   DVMRP
> redistributing routes, DVMRP
> redistribution routes
>   disabling dynamic (DVMRP)
> remote neighbors
>   PIM sparse mode
>     configuring 1, 2, 3, 4
> remote-neighbor command
> removing PIM 1, 2
> rendezvous point router. See RP routers
> reporting IP multicast groups
> reporting IPv6 multicast groups
> resetting PIM counters and mappings 1, 2
> reverse-path forwarding. See RPF
> RIP (Routing Information Protocol)
>   BFD liveness detection and 1, 2
>   detecting path failures 1, 2
>   purging learned routes 1, 2
> route-map command
> router commands
>   router dvmrp 1, 2
>   router igmp
>   router mld
>   router pim 1, 2, 3, 4
> routes
>   using for other protocols 1, 2
> routing policy commands
>   set admission-bandwidth
>   set qos-bandwidth
> RP (rendezvous point) routers
>   assigning automatically
>   configuring
>     automatic 1, 2
>     static 1, 2
> RPF (reverse-path forwarding) 1, 2, 3
> RPF routes, monitoring 1, 2

S

> set threshold command
> setting
>   baseline
>     DVMRP
>     IGMP
>     IGMP Proxy
>     MLD
>     MLD Proxy
>   DVMRP hop-count
>   PIM SPT threshold
>     IP
>     IPv6
> shared trees 1, 2, 3, 4
> shortest path trees. See SRTs
> show ip commands
>   show ip mroute
>   show ip mroute count 1, 2, 3, 4
>   show ip mroute oif-detail
>   show ip mroute summary
>   show ip rpf-route
> show ip dvmrp commands
>   show ip dvmrp
>   show ip dvmrp interface
>   show ip dvmrp mroute
>   show ip dvmrp neighbor
>   show ip dvmrp route
>   show ip dvmrp routeNextHop
> show ip igmp commands
>   show ip igmp
>   show ip igmp groups
>   show ip igmp interface
>   show ip igmp interface brief
>   show ip igmp membership
>   show ip igmp-proxy
>   show ip igmp-proxy groups
>   show ip igmp-proxy interface
> show ip multicast commands
>   show ip multicast protocols
>   show ip multicast protocols brief
>   show ip multicast routing
> show ip pim commands
>   show ip pim
>   show ip pim auto-rp
>   show ip pim bsr
>   show ip pim data-mdt
>   show ip pim dense-mode sg-state
>   show ip pim interface
>   show ip pim neighbor
>   show ip pim rp
>   show ip pim rp-hash
>   show ip pim sparse-mode sg-state
>   show ip pim sparse-mode unicast-route
>   show ip pim spt-threshold
> show ipv6 commands
>   show ipv6 mroute
>   show ipv6 mroute count 1, 2
>   show ipv6 mroute oif-detail
>   show ipv6 mroute summary
>   show ipv6 rpf-route
> show ipv6 mld commands
>   show ipv6 mld
>   show ipv6 mld groups
>   show ipv6 mld interface
>   show ipv6 mld interface brief
>   show ipv6 mld membership
>   show ipv6 mld-proxy
>   show ipv6 mld-proxy groups
>   show ipv6 mld-proxy interface
> show ipv6 mld ssm-mapping command
> show ipv6 multicast commands
>   show ipv6 multicast protocols
>   show ipv6 multicast protocols brief
>   show ipv6 multicast routing
> show ipv6 pim commands
>   show ipv6 pim
>   show ipv6 pim bsr
>   show ipv6 pim interface
>   show ipv6 pim neighbor
>   show ipv6 pim remote-neighbor
>   show ipv6 pim rp
>   show ipv6 pim rp-hash
>   show ipv6 pim sparse-mode sg-state
>   show ipv6 pim sparse-mode unicast-route
>   show ipv6 pim spt-threshold
> show multicast group limit command 1, 2
> source-rooted trees. See SRTs
> Source-Specific Multicast for IP—draft-ietf-ssm-arch-06.txt (March 2005 expiration)
> specifying IP multicast groups
> specifying IPv6 multicast groups
> SPTs (shortest path trees). See SRTs
> SRTs (source-rooted trees) 1, 2, 3, 4, 5
> static routes
>   configuring 1, 2
> summary addresses
>   DVMRP routing
> support, technical See technical support

T

> technical support
>   contacting JTAC
> text and syntax conventions
> timers
>   PIM sparse mode 1, 2
> trace packets
> tunnel group-address-pool command
> tunnel mdt command 1, 2

U

> undebug commands
>   undebug ip pim
>   undebug ipv6 pim
> unicast routes, DVMRP
> update-source command
> upstream interface 1, 2

V

> vlan commands
>   encapsulation vlan 1, 2