# Monitoring BGP/MPLS VPNs

This chapter describes how to monitor the BGP/MPLS VPN settings.

| Note: The E120 router and E320 router output for monitor and show commands is identical to output from other E Series routers, except that the E120 and E320 router output also includes information about the adapter identifier in the interface specifier (slot/adapter/port).

- Enabling the MP-BGP Events Log Display
- Monitoring BGP Next Hops for VPN
- Monitoring VRF Interfaces
- Monitoring VRF Routing Protocols
- Monitoring the VRF Routing Table
- Monitoring the VRF
- Monitoring Load-Balanced Martini Circuits
- Monitoring MPLS Tunnels
- Disabling the MP-BGP Events Log Display