Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# summary-address

#### Syntax

IS-IS:

summary-address address mask [ level-1 | level-1-2 | level-2 ] [ metric ]
[ tag tagValue ]

no summary-address address mask [ level-1 | level-1-2 | level-2 ]

OSPF:

[ no ] summary-address address mask

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates aggregate addresses for IS-IS or aggregates external routes at the border of the OSPF domain. The no version restores the default.

#### Options

- address—Summary IP address designated for a range of addresses
- mask—IP subnet mask used for the summary route
- level-1—Summarizes routes redistributed into level 1; when distributing routes domain wide, summarizes routes leaked from level 2 into level 1
- level-1-2—Summarizes routes redistributed into level 1 and level 2 IS-IS, and routes leaked between levels
- level-2—Summarizes routes learned by level 1 routing into the level 2 backbone with the configured address/mask value; also summarizes routes redistributed into level 2 IS-IS
- metric—Number in the range 1–16777215; the default metric value. The summary uses this value when advertising the summary address. When no metric is supplied, uses the value of the lowest-cost route that this is summarizing (default).
- tagValue—Number in the range 1–4294967295 that identifies the route tag assigned to the IS-IS summary address

#### Mode

Router Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out