# address network

#### Syntax

address { ipAddress | unnumbered interfaceType interfaceSpecifier }
network { broadcast | non-broadcast | point-to-point }

no address { ipAddress | unnumbered interfaceType interfaceSpecifier } network

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the OSPF network type for the specified interface to something other than the default for the network medium. The no version restores the default value for the medium.

| Note: You must issue the address area command before issuing this command.

#### Options

- ipAddress—OSPF interface address previously specified with the address command
- unnumbered—Indicates that OSPF is running on an unnumbered interface previously specified with the address command
  - interfaceType—Interface type; see Interface Types and Specifiers
  - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- broadcast—Sets network type to broadcast
- non-broadcast—Sets network type to NBMA
- point-to-point—Sets network type to point-to-point

#### Mode

Router Configuration