# query-interval

#### Syntax

query-interval queryTime

no query-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies how often the router sends PIM router query messages to remote neighbors. The no version specifies the default time interval, 30 seconds.

| Note: This command is typically used when you configure PIM remote neighbors to run multicast services over BGP/MPLS VPNs. That functionality is no longer supported.

#### Options

- queryTime—Interval, in the range 0–210 seconds, at which the router sends PIM router query messages from this interface

#### Mode

Interface Configuration