# BGP Signaling for VPWS Overview

This section describes one way to configure BGP signaling for VPWS, but does not provide complete details about configuring BGP and BGP/MPLS VPNs..

Table 134 lists the commands used in this section to configure BGP signaling for VPWS.

Table 134: Commands to Configure BGP Signaling for VPWS

address-family l2vpn | neighbor next-hop-self
address-family vpws | neighbor remote-as
exit-address-family | neighbor update-source
neighbor activate | router bgp