# frame-relay intf-type

#### Syntax

frame-relay intf-type type

no frame-relay intf-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures a Frame Relay interface type. The no version restores the default value, DTE.

#### Options

- type—One of the following interface types:
  - dce—Router is connected to user DTE equipment
  - dte—Router is connected to a Frame Relay network; the default
  - nni—Router connects two Frame Relay networks

#### Mode

Interface Configuration

#### Related Documentation

- Configuring Frame Relay Layer 2 Services in the JunosE BGP and MPLS Configuration Guide