# Switching to the Redundant SRP Module

To switch immediately from the primary SRP module to the redundant SRP module, you can use the redundancy force-switchover command or the srp switch command. You can also configure the router to prompt you if the modules are in a state that could lead to loss of configuration data or NVS corruption.

Switch from the primary SRP module to the redundant SRP module by doing either of the following:

- Issue the redundancy force-switchover command.
  host1#redundancy force-switchover 5
- Issue the srp switch force command.
  host1#srp switch force

#### Related Documentation

- Understanding SRP Module Redundancy
- Installing a Redundant SRP Module
- Managing SRP Module Redundancy
- redundancy force-switchover
- srp switch